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	OBRAZAC IZVJEŠTAJA I SADRŽAJA ISPITA PRAKTIČNE OSPOSOBLJENOSTI ZA STICANJE DOZVOLE PRIVATNOG PILOTA HELIKOPTERA – PPL(H)  
Report and Content form for the skill test for the issue of a Private Pilot Licence - PPL(H)


	IME I PREZIME KANDIDATA:

Applicant's name:
	

	TIP/BROJ DOZVOLE KANDIDATA: 

Licence type / number:
	

	NADLEŽNA DRŽAVA IZDAVANJA DOZVOLE: 

Issuing country:
	

	POTPIS KANDIDATA:
Applicant's signature:
	


-------------------------------------------------------------------------------------------------------------------------------------------------

	IME I PREZIME ISPITIVAČA: 

Examiner's name:
	

	DOZVOLA TIP/BROJ:
Licence type / number:
	

	BROJ OVLAŠTENJA I ULOGA ISPITIVAČA:

Examiner's authorisation number and role:
	

	POTPIS ISPITIVAČA:

Examiner's signature:
	


-----------------------------------------------------------------------------------------------------------------------------------------------
	NADZOR NAD PROVOĐENJEM PRAKTIČNOG DIJELA ISPITA IZVRŠIO ZRAKOPLOVNI INSPEKTOR: 

Skill test conducted under supervision of aviation inspector:
	

	POTPIS ZRAKOPLOVNOG INSPEKTORA:

Aviation inspector's signature:
	


-----------------------------------------------------------------------------------------------------------------------------------------------
	Izvještaj o provjeri praktične obučenosti / Skill test report details

	Aerodromi ili mjesto: 

Aerodromes or sites: 
	
	
	Vrijeme polijetanja: 

Take-off time:
	
	

	
	
	
	
	
	

	 Datum provjere:
Date of the test:
	
	
	Vrijeme slijetanja: 

Landing time: 
	
	

	
	
	
	
	
	

	Tip helikoptera/simulatora:

Helicopter/simulator type:
	
	Ukupno vrijeme letenja: 

Total flight time:
	

	Registracija helikoptera/simulatora:

Helicopter/simulator registration:
	

	Datum i mjesto:

Date and place:
	
	Rezultat ispita / Test result

	
	
	POLOŽIO PASS
	DJELIMIČNO POLOŽIO* PARTIAL PASS*
	NIJE POLOŽIO* 
FAIL*
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	* Razlog zašto nije položio
* reason(s) why, if failed
	

	Ime ispitivača (velikim štampanim slovima):

Examiner's name (in capital block lettters):
	Potpis ispitivača:

Examiner's signature:
	Broj certifikata ispitivača:

Examiner's certificate number
	Tip i broj dozvole:

Licence type and number:

	..................................................
	.........................
	.....................................
	.............................


SADRŽAJ PRAKTIČNOG ISPITA/PROVJERE STRUČNOSTI ZA STICANJE DOZVOLE PPL(H)
Područje i rutu leta treba da odabere ispitivač letenja (FE), a sve operacije letenja na malim visinama i lebdenja treba izvoditi na odgovarajućem aerodromu ili odgovarajućem mjestu. Rute koje se koriste za sekciju 3 mogu se završiti na aerodromu polaska ili na drugom aerodromu. Kandidat je odgovoran za planiranje leta i dužan je da osigura da se sva oprema i dokumentacija potrebna za izvršenje leta nalaze u zrakoplovu. Navigacijski dio ispita, kako je utvrđeno ovim AMC-om, treba da se sastoji od najmanje tri dionice, pri čemu svaka dionica mora trajati najmanje 10 minuta. Provjera praktične osposoblјenosti može se obaviti u dva leta.
Kandidat treba da pokaže ispitivaču letenja (FE) izvršene provjere i radnje, uklјučujući identifikaciju radio-navigacijskih sredstava. Provjere treba izvršiti u skladu sa odobrenom kontrolnom listom ili pilotskim priručnikom za korištenje helikoptera na kojem se ispit provodi. Tokom pretpoletne pripreme za ispit, kandidat je dužan da odredi postavke snage i brzine. Performanse za polijetanje, prilaženje i slijetanje kandidat treba da izračuna u skladu sa operativnim priručnikom ili letačkim priručnikom za helikopter koji se koristi.
DOZVOLJENA ODSTUPANJA TOKOM ISPITA
Kandidat tokom ispita mora da prikaže vještinu da 
1. Upravlјa helikopterom u skladu sa ograničenjima 

2. Rutinski i precizno izvršava sve manevre 

3. Dobro rasuđuje i blagovremeno donosi odluke 

4. Primjenjuje stečena zrakoplovna znanja 

5. Održava kontrolu nad helikopterom sve vrijeme na takav način da se uspješan ishod bilo kakvog postupka ili manevara nikada ne dovodi u pitanje 

Dole navedena odstupanja su opšte uputstvo za provođenje ispitnog leta. Ispitivač u toku ispitnog leta može da koriguje odstupanja ukoliko se let obavlјa u turbulenciji i u zavisnosti od upravlјivosti i performansi helikoptera:

	(1) visina:
	(i) normalan let naprijed
	± 150 ft

	
	(ii) pri simuliranom otkazu
	± 200 ft

	
	(iii) IGE lebdenje
	± 2 ft

	(2) upravlјanje u kurs ili praćenje putanje putem radio-navigacijskih sredstava:
	(i) normalan let
	± 10°

	
	(ii) pri simuliranom otkazu
	± 15° 

	(3) brzina:
	(i) polijetanje i prilaz
	+ 10/+15 čvorova

	
	(ii) svi ostali režimi leta
	± 15 čvorova

	(4) zanošenje: 


	(i) polijetanje iz IGE lebdenja 

(ii) slijetanje
	± 3 ft 

bez bočne ili leđne kretnje


Standardi uspješnog polaganja
1. Praktični ispit je podijelјen na različite sekcije koje predstavlјaju sve različite faze leta koje odgovaraju kategoriji zrakoplova na kojem se leti.

2. Ako kandidat ne položi bilo koju tačku iz jedne sekcije, smatra se da nije položio cijelu tu sekciju. Ako kandidat ne položi jednu sekciju, mora ponovo da polaže samo tu sekciju. Ako kandidat ne položi više od jedne sekcije, smatra se da nije položio cijeli ispit.

3. Ako ispit mora da bude ponovlјen u skladu sa tačkom 2, u slučaju neuspjeha iz bilo koje sekcije, uklјučujući i one koje su bile položene u prethodnom pokušaju, smatraće se da kandidat nije položio ispit u cjelini.

4. Neuspješno polaganje svih sekcija ispita iz 2 pokušaja zahtijeva dalјu praktičnu obuku kandidata.
CONTENTS OF THE SKILL TEST FOR THE ISSUE OF A PPL(H)

The area and route to be flown should be chosen by the FE and all low level and hover work should be at an adequate aerodrome or site. Routes used for section 3 may end at the aerodrome of departure or at another aerodrome. The applicant should be responsible for the flight planning and should ensure that all equipment and documentation for the execution of the flight are on board. The navigation section of the test, as set out in this AMC should consist of at least three legs, each leg of a minimum duration of 10 minutes. The skill test may be conducted in two flights

An applicant should indicate to the FE the checks and duties carried out, including the identification of radio facilities. Checks should be completed in accordance with the authorised checklist or pilot operating handbook for the helicopter on which the test is being taken. During pre-flight preparation for the test the applicant is required to determine power settings and speeds. Performance data for take-off, approach and landing should be calculated by the applicant in compliance with the operations manual or flight manual for the helicopter used.

FLIGHT TEST TOLERANCE 

The applicant should demonstrate the ability to:

1. (1) operate the helicopter within its limitations;

2. (2) complete all manoeuvres with smoothness and accuracy;

3. (3) exercise good judgement and airmanship;

4. (4) apply aeronautical knowledge;

5. (5) maintain control of the helicopter at all times in such a manner that the successful outcome of a procedure or manoeuvre is never seriously in doubt.

The following limits are for general guidance. The FE should make allowance for turbulent conditions and the handling qualities and performance of the helicopter used.

	(1) height:
	(i) normal forward flight
	± 150 ft

	
	(ii) with simulated major emergency
	± 200 ft

	
	(iii) hovering IGE flight
	± 2 ft

	(2) heading or tracking of radio aids:
	(i) normal flight
	± 10°

	
	(ii) with simulated major emergency
	± 15° 

	(3) speed:
	(i) take-off and approach
	+ 10/+15 knots

	
	(ii) all other flight regimes
	± 15 knots

	(4) round drift: 


	(i) take-off hover IGE 

(ii) landing
	± 3 ft 

no sideways or backwards movement


1. The skill test is divided into different sections, representing all the different phases of flight appropriate to the category of aircraft flown.

2. Failure in any item of a section will cause the applicant to fail the entire section. If the applicant fails only 1 section, he/she shall repeat only that section. Failure in more than 1 section will cause the applicant to fail the entire test.

3. When the test needs to be repeated in accordance with (2), failure in any section, including those that have been passed on a previous attempt, will cause the applicant to fail the entire test.

4. Failure to achieve a pass in all sections of the test in 2 attempts will require further practical training.
	Sadržaj praktičnog ispita/provjere stručnosti za sticanje dozvole PPL(H)

Upotreba ček listi, vođenje leta (letenje pomoću vizuelnih orijentira, procedure protiv zaleđivanja i razleđivanja i sl.) primjenjuju se u svim dijelovima. 

Contents of the skill test/proficiency check for the issue of a PPL(H)

Use of checklist, airmanship (control of aeroplane by external visual reference, anti/de-icing procedures, etc.) apply in all sections.
	Inicijali ispitivača nakon ispita
Examiner's initials when test completed

	
	1st

attempt
	2nd

attempt

	ODJELJAK 1 – Radnje prije polijetanja i polijetanje 
SECTION 1 -  Pre-flight operations and departure 

	a) 
	Poznavanje helikoptera (npr. Tehnička knjižica, gorivo, masa i centar težišta, performanse) planiranje leta, NOTAM, vremenski uslovi
Helicopter knowledge, (e.g. technical log, fuel, mass and balance, performance), flight planning, NOTAMs, weather briefing
	
	

	b) 
	Pretpoletni pregled/postupak, položaj dijelova i namjena 

Pre-flight inspection/action, location of parts and purpose 
	
	

	c) 
	Pregled kabine i postupak startovanja motora 

Cockpit inspection and starting procedure 
	
	

	d) 
	Provjera komunikaciјske i navigacijske opreme, izbor i podešavanje frekvencija 

Communication and navigation equipment checks, selecting and setting frequencies 
	
	

	e) 
	Postupci prije polijetanja, R/T procedure, veza sa ATC – usaglašavanje 

Pre-take-off procedure, R/T procedure, ATC compliance 
	
	

	f) 
	Parkiranje, zaustavlјanje motora i rotora i postupci poslije leta 

Parking, shutdown and post-flight procedure 
	
	

	ODJELJAK 2 –  Manevri u lebdenju, tehnika pilotiranja na ograničenim površinama 
SECTION 2 -  Nover manoeuvres, advanced handling and confined areas 

	a) 
	Polijetanje i slijetanje (uzlijetanje i pristajanje) 

Take-off and landing (lift-off and touch down) 
	
	

	b) 
	Voženje, voženje pomijeranjem iz lebdenja 

Taxi, hover taxi
	
	

	c) 
	Lebdenje u mjestu sa čeonim/bočnim/leđnim vjetrom 

Stationary hover with head/cross/tail wind 
	
	

	d) 
	Okretanje u lebdenju za 360º u lijevu i desnu stranu (u mjestu) 

Stationary hover turns, 360º left and right (spot turns) 
	
	

	e) 
	Pomijeranje naprijed, bočno, nazad 

Forward, sideways and backwards hover manoeuvring 
	
	

	f) 
	Imitacija otkaza motora u lebdenju 

Simulated engine failure from the hover 
	
	

	g) 
	Brzo zaustavlјanje u vjetar i niz vjetar 

Quick stops into and downwind 
	
	

	h) 
	Nagnuti tereni/polijetanje i slijetanje na nepripremlјene terene 

Sloping ground/unprepared sites landings and take-offs 
	
	

	i) 
	Polijetanje (različiti profili) 

Take-offs (various profiles) 
	
	

	j) 
	Polijetanje sa bočnim ili leđnim vjetrom (ako je izvodlјivo) 

Crosswind, downwind take-off (if practicable) 
	
	

	k) 
	Polijetanje sa maksimalnom poletnom masom (stvarnom i simuliranom) 

Take-off at maximum take-off mass (actual or simulated) 
	
	

	l) 
	Prilazi (različiti profili) 

Approaches (various profiles) 
	
	

	m) 
	Polijetanje i slijetanje sa ograničenom snagom 

Limited power take-off and landing 
	
	

	n) 
	Autorotacija (ispitivač bira dvije mogućnosti od – opšti postupci, dolet, na maloj brzini, u zaokretima za 360°) 

Autorotations, (FE to select two items from - basic, range, low speed, and 360º turns) 
	
	

	Potpis ispitivača:
Examiner's signature:
	


	Sadržaj praktičnog ispita/provjere stručnosti za sticanje dozvole PPL(H)

Upotreba ček listi, vođenje leta (letenje pomoću vizuelnih orijentira, procedure protiv zaleđivanja i razleđivanja i sl.) primjenjuju se u svim dijelovima. 

Contents of the skill test/proficiency check for the issue of a PPL(H)

Use of checklist, airmanship (control of aeroplane by external visual reference, anti/de-icing procedures, etc.) apply in all sections 
	Inicijali ispitivača nakon ispita
Examiner's initials when test completed

	
	1st

attempt
	2nd

attempt

	o) 
	Postupak prinudnog slijetanja sa korištenjem snage motora 

Practice forced landing with power recovery 
	
	

	p) 
	Provjere snage, tehnika praćenja, tehnika prilaza i odleta 

Power checks, reconnaissance technique, approach and departure technique 
	
	

	ODJELJAK 3 – Navigacija – postupci na ruti 
SECTION 3 - Navigation - en route procedures 

	a) 
	Navigacija i orijentacija na različitim visinama/visine, očitavanje karata 

Navigation and orientation at various altitudes/heights, map reading 
	
	

	b) 
	Održavanje visine, brzine i kursa, osmatranje zračnog prostora, podešavanje visinomjera 

Altitude/height, speed, heading control, observation of airspace, altimeter setting 
	
	

	c) 
	Praćenje leta, zapisivanje podataka, potrošnja goriva, PVD, određivanje ispravke kursa i održavanje korekcije, osmatranje instrumenata 

Monitoring of flight progress, flight-log, fuel usage, endurance, ETA, assessment of track error and re-establishment of correct track, instrument monitoring 
	
	

	d) 
	Osmatranje vremenskih uslova, proračun zaobilaženja 

Observation of weather conditions and diversion planning 
	
	

	e) 
	Upotreba radio-navigacijskih sredstava (gdje je moguće) 

Use of navigation aids (where available) 
	
	

	f) 
	Veza sa ATC i pridržavanje propisa 

ATC liaison with due observance of regulations, etc. 
	
	

	ODJELJAK 4 – Postupci u letu i manevri 
 SECTION 4 - Flight procedures and manoeuvres

	a) 
	Horizontalni let, kontrola pravca, visine i brzine 

Level flight, control of heading, altitude/height and speed 
	
	

	b) 
	Penjajući i spuštajući zaokreti sa vađenjem u određenim kursevima 

Climbing and descending turns to specified headings 
	
	

	c) 
	Lijevi i desni horizontalni zaokreti nagiba do 30º, za 180º i 360º 

Level turns with up to 30ºbank, 180º to 360º left and right 
	
	

	d) 
	Lijevi i desni standardni horizontalni zaokret za 180º, samo na osnovu pokazivanja instrumenata 

Level turns 180º left and right by sole reference to instruments 
	
	

	ODJELJAK 5 – Vanredni i postupci u slučaju opasnosti 
 SECTION 5 - Abnormal and emergency procedures 

	Napomena (1) 

	Ako se ispit provodi na višemotornom helikopteru, imitacija otkaza motora, uklјučujući prilaz i slijetanje sa jednim motorom, mora biti uklјučena u ispit. 

Where the test is conducted on a multi-engine helicopter, a simulated engine failure drill, including a single engine approach and landing, shall be included in the test. 

	Napomena (2)
	Ispitivač će odabrati 4 stavke od dole navedenih: 

The FE shall select 4 items from the following:

	a) 
	Neispravnosti rada motora, uklјučujući kvar generatora, zaleđivanje karburatora/motora, ulјnog sistema (ako je primenjivo) 

Engine malfunctions, including governor failure, carburetor/engine icing, oil system, as appropriate 
	
	

	b) 
	Neispravnost gorivnog sistema 

Fuel system malfunction 
	
	

	c) 
	Neispravnost električnog sistema 

Electrical system malfunction 
	
	

	Potpis ispitivača:

Examiner's signature:
	


	Sadržaj praktičnog ispita/provjere stručnosti za sticanje dozvole PPL(H)

Upotreba ček listi, vođenje leta (letenje pomoću vizuelnih orijentira, procedure protiv zaleđivanja i razleđivanja i sl.) primjenjuju se u svim dijelovima. 

Contents of the skill test/proficiency check for the issue of a PPL(H)

Use of checklist, airmanship (control of aeroplane by external visual reference, anti/de-icing procedures, etc.) apply in all sections 
	Inicijali ispitivača nakon ispita
Examiner's initials when test completed

	
	1st

attempt
	2nd

attempt

	d) 
	Neispravnost hidrauličnog sistema, uklјučujući prilaz i slijetanje bez servo uređaja, ako je primenjivo 

Hydraulic system malfunction, including approach and landing without hydraulics, as applicable 
	
	

	e) 
	Neispravnost glavnog rotora i/ili torkmetra (samo na simulatoru leta ili kroz usmeno objašnjavanje postupaka) 

Main rotor and/or anti-torque system malfunction (flight simulator or discussion only) 
	
	

	f) 
	Pojava požara, uklјučujući kontrolu i otklanjanje uzroka pojave dima (ako je primenjivo) 

Fire drills, including smoke control and removal, as applicable 
	
	

	g) 
	Drugi vanredni i postupci u opasnosti, kao što je opisano u odgovarajućem letačkom priručniku i u skladu sa Dodatkom 9C na PART-FCL, dijelovi 3 i 4; uklјučujući višemotorne helikoptere: 

Other abnormal and Emergency procedures as outlined in appropriate flight manual and with reference to Appendix 9C to PART-FCL, sections 3 and 4, including for multi-engine helicopters: 

a. simulirani otkaz motora u polijetanju (Simulated engine failure at take-off): 

· prekinuto polijetanje na ili prije TDP ili sigurno prinudno slijetanje na ili prije DPATO (rejected take-off at or before TDP or safe forced landing at or before DPATO); 

· ubrzo poslije LDP ili DPATO (shortly after TDP or DPATO); 

b. slijetanje sa simuliranim otkazom motora (Landing with simulated engine failure): 

· slijetanje ili produžavanje na drugi krug nakon otkaza motora prije LDP ili DPBL (landing or go-around following engine failure before LDP or DPBL);

· otkaz motora poslije LDP ili sigurno slijetanje poslije DPBL (following engine failure after LDP or safe forced landing after DPB) 
	
	

	Potpis ispitivača:

Examiner's signature:
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