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	IME I PREZIME KANDIDATA:

APPLICANT'S NAME:
	

	TIP/BROJ DOZVOLE KANDIDATA: 

LICENCE TYPE / NUMBER:
	

	POTPIS KANDIDATA:
APPLICANT'S SIGNATURE:
	


-------------------------------------------------------------------------------------------------------------------------------------------------

	IME I PREZIME INSTRUKTORA:

INSTRUCTOR'S NAME:
	

	DOZVOLA TIP/BROJ:

LICENCE TYPE / NUMBER:
	

	POTPIS INSTRUKTORA:
INSTRUCTOR'S SIGNATURE:
	


-----------------------------------------------------------------------------------------------------------------------------------------------

	IME I PREZIME ISPITIVAČA: 

EXAMINER'S NAME:
	

	DOZVOLA TIP/BROJ:
LICENCE TYPE / NUMBER:
	

	BROJ OVLAŠTENJA I ULOGA ISPITIVAČA:

AUTHORISATION NUMBER AND ROLE OF EXAMINER:
	

	POTPIS ISPITIVAČA:

EXAMINER'S SIGNATURE:
	


---------------------------------------------------------------------------------------------------------------------------------------------------------------
	A
	FFS
	FTD
	OTD
	
	Tip zrakoplova: 

Aircraft type:
	Registracija: Registration:
	Vrijeme provjere:
Total flight time:
	Datum provjere:

Date of test/check:
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Slјedeći simboli znače (The following symbols mean):
M =   obavezna vježba (mandatory exercise)

P =  osposoblјen kao PIC ili kopilot i kao pilot koji pilotira (PF) i pilot koji (trenutno) ne pilotira (PNF) za izdavanje ovlaštenja za tip kako je primjenjivo (Trained as PIC or Co-pilot and as PF and PNF for the issue of a type rating as applicable).

H =  za ove vježbe moraju da se koriste simulatori ako su na raspolaganju, u suprotnom mora da se koristi avion, ako je podesan za manevre i procedure (Simulators shall be used for this exercise, if available; otherwise an aeroplane shall be used if appropriate for the manoeuvre or procedure).

P# = obuka mora da bude dopunjena pretpoletnim pregledom aviona pod nadzorom  (The training shall be complemented by supervised aeroplane inspection).

Praktična obuka će se izvoditi na nivou opreme za obuku prikazanu kao (P), ili se može izvoditi na većem nivou opreme prikazanom strelicom (—>) (The practical training shall be conducted at least at the training equipment level shown as (P), or may be conducted up to any higher equipment level shown by the arrow (—>).

Slјedeće skraćenice se koriste za označavanje opreme (The following abbreviations are used to indicate the training equipment used):

FFS
Simulator letenja (Full Flight Simulator)

FTD
Uređaj za letačku obuku (Flight Training Device)

A
Avion (aeroplane)

Dijelovi označeni zvjezdicom (*) će se letjeti isklјučivo koristeći instrumente. Ako se ovaj uslov ne zadovolјi tokom ispita praktične osposoblјenosti ili provjere stručnosti, ovlaštenje za tip će biti ograničeno samo na VFR (The starred items (*) shall be flown solely by reference to instruments. If this condition is not met during the skill test or proficiency check, the type rating will be restricted to VFR only).

FFS će se koristiti za praktičnu obuku i ispitivanje za ovlaštenje za tip ako je FFS dio odobrenog kursa osposoblјavanja za ovlaštenje za tip. Slјedeće će biti primjenjivo za odobrenje takvog kursa (An FFS shall be used for practical training and testing if the FFS forms part of an approved type rating course. The following considerations will apply to the approval of the course):

i. kvalifikacija FFS ili FNPT II (the qualification of the FFS or FNPT II);

ii. kvalificiranost instruktora (the qualifications of the instructors);

iii. količina osposoblјavanja na FFS ili FNPT II tokom kursa i (the amount of FFS or FNPT II training provided on the course and);

iv. kvalifikacije i prethodno iskustvo na sličnim tipovima, pilota koji se osposoblјava (the qualifications and previous experience on similar types, of the pilot under training)
Manevri i procedure moraju da obuhvate saradnju višečlane posade (MSS) za avione sa više pilota i složene (complex) avione visokih performansi sa jednim pilotom u operacijama sa više pilota (Manoeuvres and procedures shall include MCC for multi-pilot aeroplane and for single-pilot high performance complex aeroplanes in multi-pilot operations). 
Manevri i procedure moraju da budu provedeni u ulozi jednog pilota za složene (complex) avione visokih performansi sa jednim pilotom u operacijama sa jednim pilotom (Manoeuvres and procedures shall be conducted in single-pilot role for single-pilot high performance complex aeroplanes in single-pilot operations). 
U slučaju složenih (complex) aviona visokih performansi sa jednim pilotom, kada se praktični ispit ili provjera stručnosti provode u operacijama sa više pilota, ovlaštenje za letenje na tipu mora da bude ograničeno na letove sa više pilota. Ako su zatražena prava za jednog pilota, manevri/procedure iz tač. 2.5, 3.9.3.4, 4.3, 5.5 i najmanje jedan manevar/procedura iz sekcije 3.4 moraju da budu dodatno izvršeni u ulozi jednog pilota (In the case of single-pilot high performance complex aeroplanes, when a skill test or proficiency check is performed in multi-pilot operations, the type rating shall be restricted to multi-pilot operations. If privileges of single-pilot are sought, the manoeuvres/procedures in 2.5, 3.9.3.4, 4.3, 5.5 and at least one manoeuvre/procedure from section 3.4 have to be completed in addition as single-pilot). 
U slučaju ograničenih ovlaštenja za letenje na tipu izdatih u skladu sa FCL.720.A (e), kandidati moraju da ispune iste zahtjeve kao ostali kandidati za ovlaštenje za letenje na tipu, izuzev vježbi koje se odnose na faze polijetanja i slijetanja (In case of a restricted type rating issued in accordance with FCL.720.A(e), the applicants shall fulfil the same requirements as other applicants for the type rating except for the practical exercises relating to the take-off and landing phases).

Za dobijanje ili zadržavanje privilegija PBN jedan prilaz mora biti RNP APCH. Ako RNP APCH nije moguć, obavlјa se u odgovarajuće opremlјenom FSTD-u (To establish or maintain PBN privileges one approach shall be an RNP APCH. Where an RNP APCH is not practicable, it shall be performed in an appropriately equipped FSTD)
	VIŠEPILOTNI AVION I JEDNOPILOTNI SLOŽENI AVION VISOKIH PERFORMANSI
MULTI-PILOT AEROPLANES AND SINGLE-PILOT HIGH-PERFORMANCE COMPLEX AEROPLANES
	PRAKTIČNA OBUKA
Practical training
	ATPL/MPL/ovlaštenje za tip ispit praktične osposoblјenosti ili provjera stručnosti 

ATPL / MPL / Type rating

Skill test / Prof. check

	Manevri / Procedure
Manoeuvres / Procedures


	
	Inicijali instruktora po završetku obuke Instructor's initials when training completed
	Provjeren na 

Checked in
	Inicijali ispitivača 
po završetku 

Ispita
Examiner's initials when test completed

	
	OTD
	FTD
	FFS
	A
	
	FFS

A
	

	
	
	
	
	
	
	
	1st

attempt
	2nd

attempt

	ODJELJAK 1

SECTION 1

	1 Priprema leta 
Flight preparation
1.1 Izračun sposobnosti 
Performance calculation
	P
	
	
	
	
	
	
	

	1.2 Vizuelni vanjski pregled aviona; lokacija svake stavke i svrha inspekcije 

Aeroplane external visual inspection; location of each item and purpose of inspection
	P#
	
	
	P
	
	
	
	

	1.3 Provjera kokpita 

Cockpit inspection
	
	P→
	→
	→
	
	
	
	

	1.4 Korištenje ček-liste prije startovanja motora, procedura startovanja, provjera radio-navigacijske opreme, provjera opreme, izbor i postavlјanje navigacijske i komunikacijske opreme 

Use of checklist prior to starting engines, starting procedures, radio and navigation equipment check, selection and setting of navigation and communication frequencies
	P→
	→
	→
	→
	
	M
	
	

	1.5 Taksiranje u skladu sa instrukcijama kontrole leta ili instruktora letenja
Taxiing in compliance with air traffic control or instructions of instructor
	
	
	P→
	→
	
	
	
	

	1.6 Pretpoletna provjera 

Before take-off checks
	
	P→
	→
	→
	
	M
	
	

	ODJELJAK 2
SECTION 2

	2 Polijetanja
Take-offs
	
	
	P→
	→
	
	
	
	

	2.1 
	Normalno polijetanje s različitim korištenjem zakrilaca, uklјučujući ubrzano polijetanje
Normal take offs with different flap settings, including expedited take-off
	
	
	
	
	
	
	
	

	2.2 
	*Instrumentalno polijetanje: prelazak na instrumentalno letenje prilikom rotacije ili neposredno nakon uzleta 

Instrument take-off; transition to instrument flight is required during rotation or immediately after becoming airborne
	
	
	P→
	→
	
	
	
	

	2.3 
	Polijetanje u uslovima bočnog vjetra 
Cross wind take-off
	
	
	P→
	→
	
	
	
	

	2.4 
	Polijetanje s maksimalnom masom polijetanja (pravo ili simulirano polijetanje s maksimalnom masom polijetanja) 
Take-off at maximum take-off mass (actual or simulated maximum take-off mass
	
	
	P→
	→
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Checked in
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	OTD
	FTD
	FFS
	A
	
	FFS

A
	

	
	
	
	
	
	
	
	1st

attempt
	2nd

attempt

	2.5 
	Polijetanje sa simulacijom otkaza motora 
Take-offs with simulated engine failure
	
	
	P→
	→
	
	
	
	

	2.5.1 
	Ubrzo nakon V2 (u avionima koji nisu odobreni kao transportna ili kao kategorija za kratke linije (commuter), otkaz motora neće se simulirati dok se ne dosegne minimalna visina od 500 ft iznad kraja staze. U avionima koji imaju iste performanse kao transportna kategorija bez obzira na masu aviona pri polijetanju i visine po gustini, instruktor može simulirati otkaz motora ubrzo nakon V2)

shortly after reaching V2 (in aeroplanes which are not certificated as transport category or commuter category aeroplanes, the engine failure shall not be simulated until reaching a minimum height of 500 ft above runway end. In aeroplanes having the same performance as a transport category aeroplane regarding take-off mass and density altitude, the instructor may simulate the engine failure shortly after reaching V2)
	
	
	
	
	
	
	
	

	2.5.2 
	* između V1 i V2 

* between V1 and V2
	
	
	P→
	→X
	
	M

FFS

Only
	
	

	2.6 
	Prekinuto polijetanje na razumnoj brzini prije dostizanja V1 
Rejected take-off at a reasonable speed before reaching V1
	
	
	P→
	→
	
	M
	
	

	ODJELJAK 3
SECTION 3

	3 
	Manevri leta i procedure 

Flight manoeuvres and procedures
	
	
	P→
	→
	
	
	
	

	3.1 
	Zaokreti sa spojlerom i bez spojlera 

Turns with and without spoilers
	
	
	
	
	
	
	
	

	3.2 
	Podrhtavanje prije i nakon kritičnog Machovog broja i ostale specifične karakteristike leta aviona (npr. Dutch roll) 
(Tuck under and Mach buffets after reaching the critical Mach number, and other specific flight characteristics of the aeroplane (e.g. Dutch Roll))
	
	
	P→
	→X 
	
	
	
	

	3.3 
	
	
	
	
	Aircraft may not be used for  his exercise
	
	
	
	

	3.4 
	Normalan rad sistema i kontrola inženjerskog panela
Engineer's panel normal operation of systems and controls
	P→
	→
	→
	→
	
	
	
	

	3.5 
	Normalne i vanredne operacije slјedećih sistema  
Normal and abnormal operations of the following systems
	
	
	P→
	→
	
	M
	A mandatory minimum of 3 abnormal shall be selected from 3.4.0 to 3.4.14 inclusive

	3.4.0
	Motor (elisa, ako je potrebno) 

Engine (if necessary, propeller)
	P→
	→
	→
	→
	
	
	
	

	3.5.1 
	Presurizacija i klimatizacija
Pressurisation and air-conditioning
	P→
	→
	→
	→
	
	
	
	

	3.5.2 
	Pitostatički sistem
Pitostatic system
	P→
	→
	→
	→
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	OTD
	FTD
	FFS
	A
	
	FFS

A
	

	
	
	
	
	
	
	
	1st

attempt
	2nd

attempt

	3.5.3 
	Sistem goriva 

Fuel system
	P→
	→
	→
	→
	
	
	
	

	3.5.4 
	Električni sistem 

Electrical system
	P→
	→
	→
	→
	
	
	
	

	3.5.5 
	Hidraulični sistem 

Hydraulic system
	P→
	→
	→
	→
	
	
	
	

	3.5.6 
	Sistem upravlјačkih komandi i trimera 
Flight control and Trim-system
	P→
	→
	→
	→
	
	
	
	

	3.5.7 
	Sistem za zaštitu od zaleđivanja i razleđivanja, grijanje vjetrobrana 

Anti- and de-icing system, Glare shield heating
	P→
	→
	→
	→
	
	
	
	

	3.5.8 
	Autopilot/Flight director
Autopilot/Flight director
	P→
	→
	→
	→
	
	M

(single pilot Only)
	
	

	3.5.9 
	Uređaj za indikaciju gubitka uzgona ili uređaj za izbjegavanje gubitka uzgona i uređaj za povećanje stabilnosti 

Stall warning devices or stall avoidance devices, and stability augmentation devices
	P→
	→
	→
	→
	
	
	
	

	3.5.10 
	Uređaj za upozorenje blizine zemlјe, meteorološki radar, radio-visinomjer, transponder 

Ground proximity warning system, Weather radar, radio altimeter, transponder
	
	P→
	→
	→
	
	
	
	

	3.5.11 
	Radio, navigacijska oprema, instrumenti, sistem upravlјanja letom 

Radio, navigation equipment, instruments, flight management system
	P→
	→
	→
	→
	
	
	
	

	3.5.12 
	Stajni trap i kočnica 

Landing gear and brake
	P→
	→
	→
	→
	
	
	
	

	3.5.13 
	Sistem pretkrilaca i zakrilaca 

Slat and flap system
	P→
	→
	→
	→
	
	
	
	

	3.5.14 
	Pomoćna pogonska grupa
Auxiliary power unit
	P→
	→
	→
	→
	
	
	
	

	3.6 
	Namjerno ostavlјeno prazno
Intentionally left blank
	
	
	
	
	
	
	
	

	3.7 
	Procedure u slučaju neispravnosti i opasnosti 

Abnormal and emergency procedures
	
	
	
	
	
	M
	A mandatory minimum of 3 items shall be selected from 3.6.1 to 3.6.9. inclusive.

	3.7.1 
	Vježbe u slučaju požara npr. motora, APU, kabine, odjelјka za teret, pilotske kabine, krila i električne mreže, uklјučujući evakuaciju 
Fire drills e.g. engine, APU, cabin, cargo compartment, flight deck, wing and electrical fires including evacuation
	
	P→
	→
	→
	
	
	
	

	3.7.2 
	Kontrola i uklanjanje dima 

Smoke control and removal
	
	P→
	→
	→
	
	
	
	

	3.7.3 
	Otkaz motora, gašenje i ponovno startovanje na sigurnoj visini 

Engine failures, shut-down and restart at a safe height
	
	P→
	→
	→
	
	
	
	

	3.7.4 
	Izbacivanje goriva (simulacija) 

Fuel dumping (simulated)
	
	P→
	→
	→
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	OTD
	FTD
	FFS
	A
	
	FFS

A
	

	
	
	
	
	
	
	
	1st

attempt
	2nd

attempt

	3.7.5 
	Smicanje vjetra u fazi polijetanja / slijetanja 

Windshear at take-off / landing
	
	
	P
	X
	
	FFS 

only
	
	

	3.7.6 
	Simulacija pada pritiska u kabini aviona/vanredno snižavanje 

Simulated cabin pressure failure / Emergency descent
	
	
	P→
	→
	
	
	
	

	3.7.7 
	Nesposobnost jednog od članova letačke posade 

Incapacitation of flight crew member
	
	P→
	→
	→
	
	
	
	

	3.7.8 
	Ostale procedure vanrednih situacija kako je istaknuto u odgovarajućem Letačkom priručniku 

Other emergency procedures as outlined in the appropriate aeroplane Flight Manual
	
	P→
	→
	→
	
	
	
	

	3.7.9 
	ACAS događaj 

ACAS event
	P→
	→
	→
	An Aircraft may

not be used
	
	FFS 

only
	
	

	3.8 
	Oštri zaokret s 45( nagiba,  za 180( do 360( lijevi i desni 

Steep turns with 45° bank, 180° to 360° left and right
	
	P→
	→
	→
	
	
	
	

	3.9 
	Rano prepoznavanje i mjere protiv prevlačenja aviona. Do aktiviranja sistema za upozorenje približavanja uglu gubitka uzgona u konfiguraciji za polijetanje (zakrilca u poziciji polijetanja), u konfiguraciji krstarenja za slijetanje (zakrilca u konfiguraciji za slijetanje, izvučen stajni trap) 

Early recognition and counter measures on approaching stall (up to activation of stall warning device) in take-off configuration (flaps in take-off position), in cruising flight configuration and in landing configuration (flaps in landing position, gear extended)
	
	
	P→
	→
	
	
	
	

	3.9.1 
	Izlazak iz potpunog prevlačenja aviona ili poslije aktiviranja upozorenja za približavanje kritičnom napadnom uglu u režimu penjanja, krstarenja i konfiguraciji za slijetanje 

Recovery from full stall or after activation of stall warning device in climb, cruise and approach configuration
	
	
	P
	X
	
	
	
	

	3.10 
	Procedure instrumentalnog letenja 

Instrument flight procedures
	
	
	
	
	
	
	
	

	3.10.1 
	* Pridržavanje odlaznih i dolaznih ruta i instrukcije ATC 

* Adherence to departure and arrival routes and ATC instructions
	
	P→
	→
	→
	
	M
	
	

	3.10.2 
	* Procedure kruga čekanja 

Holding procedures
	
	P→
	→
	→
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	OTD
	FTD
	FFS
	A
	
	FFS

A
	

	
	
	
	
	
	
	
	1st

attempt
	2nd

attempt

	3.10.3 
	3D operacije do DH/A od 200 stopa (60 m) ili do viših minimuma ako su određeni postupkom prilaza
NAPOMENA: U skladu sa AFM-om, RNP APCH postupci mogu zahtijevati upotrebu autopilota ili sistema za upravlјanje letom. Postupak  ručnog upravlјanja bira se uzimajući u obzir takva ograničenja (na primjer: odaberite ILS za 3.9.3.1. u slučaju takvog ograničenja u AFM-u)

3D operations to DH/A of 200 feet (60 m) or to higher minima if required by the approach procedure.

Note: According to the AFM, RNP APCH procedures may require the use of autopilot or Flight director. The procedure to be flown manually shall be chosen taking into account such limitations (for example, choose an ILS for 3.9.3.1 in case of such AFM limitation).
	
	
	
	
	
	
	
	

	3.10.3.1 
	*Ručno upravlјanje, bez uređaja za upravlјanje letom
Manually, without flight director
	
	
	P→
	→
	
	M

(skill test only)
	
	

	3.10.3.2 
	*Ručno upravlјanje, sa  uređajem za upravlјanje letom  

Manually, with flight director
	
	
	P→
	→
	
	
	
	

	3.10.3.3 
	*Automatski sa autopilotom 

With autopilot
	
	
	P→
	→
	
	
	
	

	3.10.3.4 
	Ručno, simulacijom otkaza jednog motora; simulacija otkaza motora traje za vrijeme završnog prilaza prije prelaska 1 000  stopa iznad nivoa aerodroma do dodira s tlom ili završetka postupka neuspjelog prilaza.
U avionu koji nije odobren kao transportna kategorija aviona (JAR/FAR  25) ili kao ‚commuter’ kategorija aviona (SFAR 23), prilaz sa simuliranim otkazom motora i postupkom prekinutog prilaza započinje se u skladu sa NDB ili VOR prilazom opisanim u 3.9.4. Postupak prekinutog prilaza započinje se prilikom dolaska na dozvolјenu visinu u odnosu na prepreku (obstacle clearence height) (OCH/A), ali ne kasnije od dolaska na minimalnu visinu snižavanja (MDH/A) od 500 stopa iznad nadmorske visine početka uzletno-sletne staze. U avionu koji ima jednake karakteristike kao transportna kategorija aviona u smislu uzletne mase i visine korigovane po gustoći, instruktor može simulirati otkaz motora u skladu sa 3.9.3.4.

Manually, with one engine simulated inoperative; engine failure has to be simulated during final approach before passing 1 000 feet above aerodrome level until touchdown or through the complete missed approach procedure.

In aeroplanes which are not certificated as transport category aeroplanes (JAR/ FAR 25) or as commuter category aeroplanes (SFAR 23), the approach with simulated engine failure and the ensuing go-around shall be initiated in conjunction with the non-precision approach as described in 3.9.4. The go-around shall be initiated when reaching the published obstacle clearance height (OCH/A), however not later than reaching a minimum descent height/altitude (MDH/A) of 500 feet above runway threshold elevation. In aeroplanes having the same performance as a transport category aeroplane regarding take-off mass and density altitude, the instructor may simulate the engine failure in accordance with 3.9.3.4.
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	3.10.4 
	* Neprecizni prilaz do MDH/A 2D operacije do MDH/A

* Non-precision approach to MDH/A - 2D operations down to the MDH/A
	
	
	
	
	
	
	
	

	3.10.5 
	Krug prilaženja pod slјedećim uslovima: 
Circling approach under following conditions:

(a)* prilaz do minimalne dopuštene visine za krug prilaženja na dotičnom aerodromu u skladu s lokalnim instrumentalnim prilaznim sredstvima u simuliranim instrumentalnim uslovima leta 

approach to the authorised minimum circling approach altitude at the aerodrome in question in accordance with the local instrument approach facilities in simulated instrument flight conditions;

nakon koga slijedi: 

followed by:

(b) krug prilaženja na drugu stazu za slijetanje najmanje 900 od srednje linije završnog prilaza koji se koristi u tački (a), na minimalnoj dopuštenoj visini kruga prilaženja 

circling approach to another runway at least 90° off centreline from final approach used in item (a), at the authorised minimum circling approach altitude)

Primjedba: ako (a) i (b) nije moguće izvesti iz razloga ATC, može se izvesti simulirani niski vizuelni krug prilaženja 

Remark: if (a) and (b) are not possible due to ATC reasons a simulated low visibility pattern may be performed.
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	ODJELJAK 4
SECTION 4

	4 
	Procedura neuspjelog prilaza 

Missed Approach Procedures
	
	
	
	
	
	
	
	

	4.1 
	Postupak prekinutog prilaza sa svim motorima operativnim* tokom 3D operacije prilikom dostizanja visine odluke
Go-around with all engines operating* during a 3D operation on reaching decision height
	
	
	P*→
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	4.2 
	Ostale procedure neuspjelog prilaza 

Other missed approach procedures
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	4.3 
	* Ručna procedura prekinutog prilaza sa simuliranim otkazom kritičnog motora poslije instrumentalnog prilaza do dostizanja DH, MDH ili MAPt 

* Manual go-around with the critical engine simulated inoperative after an instrument approach on reaching DH, MDH or MAPt
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	4.4 
	Prekinuto slijetanje na 15 m (50 ft) iznad početka staze i procedura prekinutog prilaza 

Rejected landing at 15 m  (50 ft) above runway threshold and go-around
	
	
	P*→
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	ODJELJAK 5
SECTION 5

	5 
	Slijetanja 

Landings
	
	
	
	
	
	
	
	

	5.1 
	Normalna slijetanja* s vizuelnom referencom uspostavlјenom na DA/H nakon operacije instrumentalnog prilaza 

Normal landings* with visual reference established when reaching DA/H following an instrument approach operation
	
	
	P
	
	
	
	
	

	5.2 
	Slijetanje sa simulacijom zaglavlјenja horizontalnog stabilizatora u bilo kom položaju koji nije onaj na koji je podešen
Landing with simulated jammed horizontal stabiliser in any out-of-trim position
	
	
	P→
	An aircraft may not be used for this exercise
	
	
	
	

	5.3 
	Slijetanje s bočnim vjetrom (avion) 

Cross wind landings (aeroplane)
	
	
	P→
	→
	
	
	
	

	5.4 
	Školski krug i slijetanje bez izvučenih ili djelimično izvučenih zakrilaca i pretkrilaca 

Traffic pattern and landing without extended or with partly extended flaps and slats
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	5.5 
	Slijetanje sa simulacijom kritičnog otkaza motora 

Landing with critical engine simulated inoperative
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	M
	
	

	5.6 
	Slijetanje sa simulacijom otkaza dvaju motora: 

Landing with two engines inoperative:

· avion s tri motora: centralni i jedan vanjski motor koliko je to moguće u skladu s podacima iz AFM 
Aeroplanes with three engines: the centre engine and one outboard engine as far as practicable according to data of the AFM)

· avion s četiri motora: dva motora na jednoj strani 

Aeroplanes with four engines, two engines at one side)
	
	
	
	
	
	M
FFS only
(skill test only)
	
	

	Opšta napomena:   Specijalni zahtjevi za proširenje ovlaštenja za tip za instrumentalne prilaze do visine odluke manje od 200 stopa (60 m), npr. CAT  II/III operacije.
General remarks:      Special requirements for extension of a type rating for instrument approaches down to a decision height of less than 200 feet (60 m), i.e. Cat II/III operations.
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	ODJELJAK 6
SECTION 6

	6 
	Ovlaštenje za tip za instrumentalne prilaze na visinu manju od 60 m (200ft)(CATII/III).

Slјedeći manevri i procedure su minimalni uslovi za obuku za odobrenje instrumentalnog prilaza na DH manju od 60 m (200 ft). Tokom slјedećih instrumentalnih prilaza i procedura prekinutog slijetanja koristiće se sva oprema aviona potrebna za izdavanje potvrde tipa za instrumentalni prilaz na DH manju od 60 m (200 ft)

Type rating for instrument approaches down to a decision height of less than 60 m (200 ft) (CAT II/III). 
The following manoeuvres and procedures are the minimum training requirements to permit instrument approaches down to a DH of less than 60 m (200 ft). During the following instrument approaches and missed approach procedures all aeroplane equipment required for type certification of instrument approaches down to a DH of less than 60 m (200 ft) shall be used.
	
	
	
	
	
	
	
	

	6.1 
	* Prekinuto polijetanje na minimalno dopuštenom RVR 

* Rejected take-off at minimum authorised RVR
	
	
	P*→
	→X
	
	M*
	
	

	6.2 
	
	
	
	
	An aircraft may not be used for this exercise
	
	
	
	

	6.3 
	CAT II/III Prilaz: U simuliranim instrumentalnim uslovima leta do primjenjive DH, koristeći se sistemom za navođenje. Standardne procedure za koordinaciju posade (SOP) će se kontrolirati.

CAT II/III approaches: In simulated instrument flight conditions down to the applicable DH, using flight guidance system. Standard procedures of crew coordination (task sharing, call out procedures, mutual surveillance, information exchange and support) shall be observed
	
	
	P→
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	6.4 
	Prekinuti prilaz: Poslije prilaza kako je prikazano u 6.2 prilikom dostizanja DH. Obuka će uklјučivati i proceduru prekinutog prilaza zbog (simuliranog) nedovolјnog RVR, smicanja vjetra, skretanja zrakoplova izvan granica prilaza za uspješan prilaz, otkaz zemalјske/avionske opreme prije dostizanja DH i procedura prekinutog prilaza sa simuliranim otkazom opreme u avionu.

Go-around: after approaches as indicated in 6.2 on reaching DH. The training shall also include a go-around due to (simulated) insufficient RVR, wind shear, aeroplane deviation in excess of approach limits for a successful approach, and ground/airborne equipment failure prior to reaching DH and, go-around with simulated airborne equipment failure
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	6.5 
	Slijetanje(a) s vizuelnom referencom uspostavlјenom na DH koja slijedi nakon instrumentalnog prilaza. U zavisnosti od specifičnog sistema navođenja, obavlјaće se automatsko slijetanje.

Landing(s): With visual reference established at DH following an instrument approach. Depending on the specific flight guidance system, an automatic landing shall be performed
	
	
	P→
	→
	
	M*
	
	


Primjedba: 
CAT II/III operacije se trebaju provesti u skladu sa odgovarajućim zahtjevima zračnog prometa.
Note: 

CAT II/III operations shall be accomplished in accordance with the applicable air operations requirements.
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