	Obrazac izvještaja i sadržaja ispita praktične osposobljenosti za sticanјe dozvole privatnog pilota aviona – PPL(A)
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	OBRAZAC IZVJEŠTAJA I SADRŽAJA ISPITA PRAKTIČNE OSPOSOBLJENOSTI ZA STICANJE DOZVOLE PRIVATNOG PILOTA AVIONA – PPL(A)
Report and Content form for the skill test for the issue of a Private Pilot Licence – PPL(A)


	IME I PREZIME KANDIDATA:

Applicant's name:
	

	TIP/BROJ DOZVOLE KANDIDATA: 

Licence type / number:
	

	NADLEŽNA DRŽAVA IZDAVANJA DOZVOLE: 

Issuing country:
	

	POTPIS KANDIDATA:

Applicant's signature:
	


-------------------------------------------------------------------------------------------------------------------------------------------------

	IME I PREZIME ISPITIVAČA: 

Examiner's name:
	

	DOZVOLA TIP/BROJ:

Licence type / number:
	

	BROJ OVLAŠĆENJA I ULOGA ISPITIVAČA:

Examiner's authorisation number and role:
	

	POTPIS ISPITIVAČA:

Examiner's signature:
	


-----------------------------------------------------------------------------------------------------------------------------------------------
	NADZOR NAD PROVOĐENJEM PRAKTIČNOG DIJELA ISPITA IZVRŠIO ZRAKOPLOVNI INSPEKTOR: 

Skill test conducted under supervision of aviation inspector:
	

	POTPIS ZRAKOPLOVNOG INSPEKTORA:

Aviation inspector's signature:
	


-----------------------------------------------------------------------------------------------------------------------------------------------
	Izvještaj o provjeri praktične obučenosti / Skill test report details

	Aerodromi: 

Aerodromes: 
	
	
	Vrijeme polijetanja: 

Take-off time:
	
	

	
	
	
	
	
	

	Datum provjere
Date of the test
	
	
	Vrijeme slijetanja: 

Landing time: 
	
	

	
	
	
	
	
	

	Tip aviona/simulatora:

Aeroplane/simulator type:
	
	Ukupno vrijeme letenja: 

Total flight time:
	

	Registracija aviona/simulatora:

Aeroplane/simulator registration:
	

	Datum i mjesto:

Date and place:
	
	Rezultat ispita / Test result

	
	
	POLOŽIO PASS
	DJELIMIČNO POLOŽIO* PARTIAL PASS*
	NIJE POLOŽIO* 
FAIL*
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	* Razlog zašto nije položio
* reason(s) why, if failed
	

	Ime ispitivača (velikim štampanim slovima):

Instructor's name (in capital block lettters):
	Potpis ispitivača:

Instructor's signature:
	Broj certifikata ispitivača:

Examiner's certificate number
	Tip i broj dozvole:

Licence type and number:

	..................................................
	.........................
	.....................................
	.............................


SADRŽAJ PRAKTIČNOG ISPITA/PROVJERE STRUČNOSTI ZA STICANJE DOZVOLE PPL(A)
Ispitnu rutu bira ispitivač. Ispitna ruta može biti završena na aerodromu polijetanja ili na drugom aerodromu. Kandidat je dužan da osigura da se sva neophodna dokumentacija i oprema za izvođenje leta nalazi u avionu i odgovoran je za planiranje letenja. Neophodno je da vrijeme trajanja navigacijskog dijela ispitnog leta bude dovolјno kako bi kandidat demonstrirao sposobnost da uspješno odleti rutu sa najmanje tri prekretne tačke. Navigacijski dio ispitnog leta, ukoliko postoji dogovor između kandidata i ispitivača, može biti proveden posebno.

Kandidat treba da pokaže ispitivaču da su sve provjere i dužnosti za izvršenje leta provedene, uklјučujući identifikaciju radio sredstava. Provjere treba da budu izvršene u skladu sa letačkim priručnikom ili u skladu sa odobrenim listama provjere za avion koji će biti korišten na ispitu. Tokom pripreme leta kandidat je dužan da odredi podešavanje snage motora i brzina. Kandidat je dužan da izvrši proračun performansi aviona na polijetanju, prilazu i slijetanju u skladu sa letačkim priručnikom aviona koji će biti korišten na ispitu.
Dozvolјena odstupanja tokom ispita
Kandidat tokom ispita mora da prikaže vještinu da 
1. Upravlјa avionom u skladu sa ograničenjima 

2. Rutinski i precizno izvršava sve manevre 

3. Dobro rasuđuje i blagovremeno donosi odluke 

4. Primjenjuje stečena zrakoplovna znanja 

5. Održava kontrolu nad avionom sve vrijeme na takav način da se uspješan ishod bilo kakvog postupka ili manevara nikada ne dovodi u pitanje 

Dole navedena odstupanja su opšte uputstvo za provođenje ispitnog leta. Ispitivač u toku ispitnog leta može da koriguje odstupanja ukoliko se let obavlјa u turbulenciji i u zavisnosti od upravlјivosti i performansi aviona:
	(1) visina
	(i) normalan let
	± 150 ft

	
	(ii) sa otkazom motora
	± 200 ft (ukoliko se koristi ME avion)

	(2) održavanje kursa
	(i)  normalan let
	± 10°

	
	(ii) sa otkazom motora
	± 15° (ukoliko se koristi ME avion)

	(3) brzina
	(i) polijetanje i prilaz
	+15/–5 čvorova

	
	(ii) svi ostali režimi leta
	±15 čvorova


Standardi uspješnog polaganja
1. Praktični ispit je podijelјen na različite sekcije koje predstavlјaju sve različite faze leta koje odgovaraju kategoriji zrakoplova na kojem se leti.

2. Ako kandidat ne položi bilo koju tačku iz jedne sekcije, smatra se da nije položio cijelu tu sekciju. Ako kandidat ne položi jednu sekciju, on mora ponovo da polaže samo tu sekciju. Ako kandidat ne položi više od jedne sekcije, smatra se da nije položio cijeli ispit.

3. Ako ispit mora da bude ponovlјen u skladu sa tačkom 2, u slučaju neuspjeha iz bilo koje sekcije, uklјučujući i one koje su bile položene u prethodnom pokušaju, smatraće se da kandidat nije položio ispit u cjelini.

4. Neuspješno polaganje svih sekcija ispita iz dva pokušaja zahtijeva dalјu praktičnu obuku kandidata.

CONTENTS OF THE SKILL TEST / PROFICIENCY CHECK FOR THE ISSUE OF A PPL(A)
The route to be flown for the navigation test should be chosen by the FE. The route may end at the aerodrome of departure or at another aerodrome. The applicant should be responsible for the flight planning and should ensure that all equipment and documentation for the execution of the flight are on board. The navigation section of the test should have a duration that allows the pilot to demonstrate his/her ability to complete a route with at least three identified waypoints and may, as agreed between the applicant and FE, be flown as a separate test. 

An applicant should indicate to the FE the checks and duties carried out, including the identification of radio facilities. Checks should be completed in accordance with the authorised checklist for the aeroplane on which the test is being taken. During pre-flight preparation for the test the applicant should be required to determine power settings and speeds. Performance data for take-off, approach and landing should be calculated by the applicant in compliance with the operations manual or flight manual for the aeroplane used.
FLIGHT TEST TOLERANCES 

The applicant should demonstrate the ability to: 
1. operate the aeroplane within its limitations 

2. complete all manoeuvres with smoothness and accuracy; 

3. exercise good judgment and airmanship;

4. apply aeronautical knowledge;

5. maintain control of the aeroplane at all times in such a manner that the successful outcome of a procedure or manoeuvre is never seriously in doubt.

The following limits are for general guidance. The FE should make allowance for turbulent conditions and the handling qualities and performance of the aeroplane used:

	(1) height:
	(i) normal flight
	± 150 ft

	
	(ii) with simulated engine failure
	± 200 ft (if ME aeroplane is used)

	(2) heading or tracking of radio aids:
	(i) normal flight
	± 10°

	
	(ii) with simulated engine failure
	± 15° (if ME aeroplane is used)

	(3) speed:
	(i) take-off and approach
	+15/–5 knots

	
	ii) all other flight regimes
	±15 knots


PASS STANDARDS

1. The skill test is divided into different sections, representing all the different phases of flight appropriate to the category of aircraft flown.

2. Failure in any item of a section will cause the applicant to fail the entire section. If the applicant fails only 1 section, he/she shall repeat only that section. Failure in more than 1 section will cause the applicant to fail the entire test.

3. When the test needs to be repeated in accordance with (2), failure in any section, including those that have been passed on a previous attempt, will cause the applicant to fail the entire test.

4. Failure to achieve a pass in all sections of the test in 2 attempts will require further practical training.

	Sadržaj praktičnog ispita/provjere stručnosti za sticanje dozvole PPL(A)

Upotreba ček listi, vođenje leta (letenje pomoću vizuelnih orijentira, procedure protiv zaleđivanja i razleđivanja i sl.) primjenjuju se u svim dijelovima. 

Contents of the skill test/proficiency check for the issue of a PPL(A)

Use of checklist, airmanship (control of aeroplane by external visual reference, anti/de-icing procedures, etc.) apply in all sections 
	Inicijali ispitivača nakon ispita
Examiner's initials when test completed

	
	1st

attempt
	2nd

attempt

	ODJELJAK 1 – Radnje prije polijetanja i polijetanje 
SECTION 1 -  Pre-flight operations and departure 

	a) 
	Pretpoletna dokumentacija, NOTAM i procjena meteo situacije 

Pre-flight documentation, NOTAM and weather briefing 
	
	

	b) 
	Proračuni performansi, težine i centraže 

Mass and balance and performance calculation 
	
	

	c) 
	Pregled i opsluživanje aviona 

Aeroplane inspection and servicing 
	
	

	d) 
	Procedure prije i poslije pokretanja motora 

Engine starting and after starting procedures 
	
	

	e) 
	Voženje, aerodromske procedure i pretpoletne procedure 

Taxiing and aerodrome procedures, pre-take-off procedures 
	
	

	f) 
	Provjere prije i poslije polijetanja 

Take-off and after take-off checks 
	
	

	g) 
	Aerodromske procedure odlaska 

Aerodrome departure procedures 
	
	

	h) 
	ATS komunikacija, procedure radio-telefonije 

ATC compliance and R/T procedures 
	
	

	ODJELJAK 2 – Opšte upravlјanje avionom 
SECTION 2 -  General Airwork 

	a) 
	ATS komunikacija, procedure radio-telefonije 

ATC compliance and R/T procedures
	
	

	b) 
	Pravolinijski horizontalni let, sa promjenama brzine 

Straight and level flight, with speed changes 
	
	

	c) 
	Penjanje / Climbing: 
i. Sa najvećom vertikalnom brzinom / Best rate of climb 
ii. Penjući zaokreti / Climbing turns 
iii. Prevođenje u horizontalni let / Levelling off 
	
	

	d) 
	Blagi zaokreti (nagiba 30º) 

Medium (30° bank) turns 
	
	

	e) 
	Oštri zaokreti (nagiba 45º) uklјučujući i prepoznavanje i vađenje iz poniruće spirale 

Steep (45° bank) turns (including recognition and recovery from a spiral dive) 
	
	

	f) 
	Let na kritično malim brzinama sa ili bez zakrilaca 

Flight at critically low airspeed with and without flaps 
	
	

	g) 
	Prevlačenje / Stalling: 

i. sa čistom konfiguracijom i vađenje sa snagom motora / Clean stall and recover with power

ii. do prvih predznaka u ponirućem zaokretu nagiba 20º, u prilaznoj konfiguraciji / Approach to stall descending turn with bank angle 20°, approach configuration
iii. do prvih predznaka u sletnoj konfiguraciji / Approach to stall in landing configuration 
	
	

	h) 
	Poniranje / Descending: 

Sa i bez snage motora / With and without engine power
Ponirući zaokreti (oštri zaokreti, bez snage motora) / Descending turns (steep gliding turns)
Prevođenja u horizontalni let / Levelling off
	
	

	Potpis ispitivača:
Examiner's signature:
	


	Sadržaj praktičnog ispita/provjere stručnosti za sticanje dozvole PPL(A)

Upotreba ček listi, vođenje leta (letenje pomoću vizuelnih orijentira, procedure protiv zaleđivanja i razleđivanja i sl.) primjenjuju se u svim dijelovima. 

Contents of the skill test/proficiency check for the issue of a PPL(A)

Use of checklist, airmanship (control of aeroplane by external visual reference, anti/de-icing procedures, etc.) apply in all sections 
	Inicijali ispitivača nakon ispita
Examiner's initials when test completed

	
	1st

attempt
	2nd

attempt

	ODJELJAK 3 – Procedure na rutama 
SECTION 3 - En-route procedures 

	a) 
	Plan leta, računska navigacija i čitanje navigacijske karte 

Flight plan, dead reckoning and map reading 
	
	

	b) 
	Održavanje visine, pravca i brzine 

Maintenance of altitude, heading and speed
	
	

	c) 
	Orijentacija, mjerenje vremena i ispravlјanje PVD, vođenje plana leta 

Orientation, timing and revision of ETAs, log keeping 
	
	

	d) 
	Procedure odlaska na alternativni aerodrom (planirane i primjenjene) 

Diversion to alternate aerodrome (planning and implementation) 
	
	

	e) 
	Upotreba radio-navigacijskih sredstava 

Use of radio navigation aids 
	
	

	f) 
	Osnovno letenje pomoću instrumenata (zaokret za 180º u simuliranim IMC) 

Basic instrument flying check (180° turn in simulated IMC) 
	
	

	g) 
	Upravlјanje letom (provjere, gorivni sistemi i zaleđivanje karburatora, itd.) 

Flight management (checks, fuel systems and carburettor icing, etc.) 
	
	

	h) 
	ATS komunikacija, procedure radio-telefonije 

ATC compliance and R/T procedures
	
	

	ODJELJAK 4 – Procedure prilaza i slijetanja 

SECTION 4 - Approuch and landing procedures 

	a) 
	Procedure dolaska na aerodrom 

Aerodrome arrival procedures 
	
	

	b) 
	*Procedure dolaska na aerodrom 

*Aerodrome arrival procedures 
	
	

	c) 
	*Slijetanje bez zakrilaca 

* Flapless landing 
	
	

	d) 
	*Prilaz za slijetanje sa snagom motora na relantu (samo jednomotorni avioni) 

* Approach to landing with idle power (Single-engine only) 
	
	

	e) 
	Slijetanje sa produžavanjem 

Touch and go 
	
	

	f) 
	Produžavanje sa male visine 

Go-around from low height 
	
	

	g) 
	ATS komunikacija, procedure radio-telefonije 

ATC compliance and R/T procedures
	
	

	h) 
	Radnje poslije letenja 
Actions after flight 
	
	

	Potpis ispitivača:
Examiner's signature:
	


	Sadržaj praktičnog ispita/provjere stručnosti za sticanje dozvole PPL(A)

Upotreba ček listi, vođenje leta (letenje pomoću vizuelnih orijentira, procedure protiv zaleđivanja i razleđivanja i sl.) primjenjuju se u svim dijelovima. 

Contents of the skill test/proficiency check for the issue of a PPL(A)

Use of checklist, airmanship (control of aeroplane by external visual reference, anti/de-icing procedures, etc.) apply in all sections 
	Inicijali ispitivača nakon ispita
Examiner's initials when test completed

	
	1st

attempt
	2nd

attempt

	ODJELJAK 5 - Vanredni i postupci u slučaju opasnosti  

(ovaj dio može da se kombinuje sa dijelovima od 1 do 4)
SECTION 5 - Abnormal and emergency procedures (This section may be combined with Sections 1 through 4)

	a) 
	Simulirani otkaz motora nakon polijetanja (samo jednomotorni avioni) 

Simulated engine failure after take-off (Single-engine only) 
	
	

	b) 
	* Simulirano prinudno slijetanje (samo jednomotorni avioni) 

* Simulated forced landing (Single-engine only) 
	
	

	c) 
	Simulirano slijetanje iz predostrožnosti (samo jednomotorni avioni) 

Simulated precautionary landing (Single-engine only) 
	
	

	d) 
	Usmena pitanja 

Oral questions 
	
	

	ODJELKAK 6 - Vanredni i postupci u slučaju opasnosti  

(ovaj dio može da se kombinuje sa dijelovima od 1 do 5)
SECTION 6 - Abnormal and emergency procedures (This section may be combined with Sections 1 through 5)

	a) 
	Simulirani otkaz motora tokom polijetanja (na sigurnoj visini osim ukoliko se izvodi na FFS) 

Simulated engine failure during take-off (at a safe altitude unless carried out in an FFS) 
	
	

	b) 
	Nesimetrični prilaz i produžavanje na drugi krug 

Asymmetric approach and go-around 
	
	

	c) 
	Nesimetrični prilaz i slijetanje sa zaustavlјanjem 

Asymmetric approach and full stop landing 
	
	

	d) 
	Gašenje motora i ponovno pokretanje 

Engine shutdown and restart 
	
	

	e) 
	ATS komunikacija, procedure radio-telefonije 

ATC compliance and R/T procedures
	
	

	f) 
	Bilo koja stavka sa praktičnog ispita koju odredi ispitivač u vezi sa praktičnom provjerom osposoblјenosti za klasu/tip, ukoliko se primjenjuje: 

i. Sistemi aviona, uklјučujući korištenje auto-pilota 

ii. Upravlјanje sistemom presurizacije 

iii. Upotreba sistema protiv odleđivanja i sistema za odleđivanje 

As determined by the Flight Examiner – any relevant items of the class/type rating skill test to include, if applicable: 

i. Aeroplane systems including handling of auto pilot 

ii. Operation of pressurisation system 

iii. Use of de-icing and anti-icing system 


	
	

	g) 
	Usmena pitanja 

Oral questions
	
	

	*neke od ovih stavki se mogu kombinirati po diskrecionoj odluci ispitivača 

*some of these items may be combined at the discretion of the Flight Examiner

	Potpis ispitivača:
Examiner's signature:
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